Release notes

A few bug fixes were necessary:

* The unit of the base type XyzVectorAndAccuracy depends on the usage in a composite type. For the resolution this was described in the architecture document, but not for unit and range.
* Fix documentation of resolution of RoadAttribution > InclinationAndCurvature > horizontal\_curvature\_and\_accuracy.
* Description for THREE\_D for NavigationSatelliteSystemStatus of VehiclePositionAndOrientation is fixed.